Filetype: Flipper SubGhz Setting File
Version: 1

# Add Standard frequencies for your region
#add_standard_frequencies: true

# Default Frequency: used as default for "Read" and "Read Raw"
#default_frequency: 433920000

# Frequencies used for "Read", "Read Raw" and "Frequency Analyzer"
#frequency: 300000000
#frequency: 310000000
#frequency: 320000000

# Frequencies used for hopping mode (keep this list small or flipper will miss signal)
#hopper_frequency: 300000000
#hopper_frequency: 310000000
#hopper_frequency: 310000000
