# for adding manufacture keys
# AABBCCDDEEFFAABB:X:NAME\r\n
# AABBCCDDEEFFAABB - man 64 bit
# X - encryption method 1 - Simple Learning, 2 - Normal_Learning, 3 - Secure_Learning,  4 - Magic_xor_type1 Learning
#   	0 - iterates over both previous and man in direct and reverse byte sequence
# NAME - name (string without spaces) max 64 characters long
Filetype: Flipper SubGhz Keystore File
Version: 0
Encryption: 0
AABBCCDDEEFFAABB:1:Test1
AABBCCDDEEFFAABB:1:Test2
